**DIS089 Assembly Instructions**

With the machine turned OFF, remove the backglass from the game

Disconnect the one ribbon cable and 2 molex connectors from the top of the original display.

Swing the display assembly down onto the top of the playfield glass.

Remove the 4 screws that attach the old display to the display assembly, and do not use again.

Attach the ribbon cable to the new DIS089 (before attaching the DIS200 to the assembly).

Attach the DIS089 to the display assembly using the 4 screws included (not the original).

Attach the two cables to the molex connectors on the back of the DIS089.

Swing the display assembly back in the upright position.

Re-attach the backglass.

You are now ready to play!